
APAR= II09782
PROBLEMS WITH OS/400 UPGRADES OF CLIENT ACCESS FOR WINDOWS 3.1


** Last updated 10/10/96 **

If you use Client Access for Windows 3.1, you should perform
the actions in this topic to prevent problems later in the
upgrade.

o If you use Client Access for Windows 3.1 in a double-byte
  language (DBCS), you may need to apply PTFs to prevent a
  problem when installing V3R7M0 OS/400-Host Servers.


Do the following BEFORE installing the new release of OS/400:

STEP 1: If you have the V3R1M1 level of 5763-XC1 installed,
        you do not need to apply these PTFs.  You do not need
        to use this procedure.  If you have the V3R1M0 level
        installed, continue with the next step.

STEP 2: Check to see if the following PTF (or a PTF that
        supersedes it) is applied.  If the PTF is installed,
        no additional action is needed.  If the PTF is not
        applied, continue with Step 3.

        The 5763-XC1 V3R1M0 PTFs are:

            SF27383
            SF35419

STEP 3: Apply the PTFs.


Continue with your planning for installing software.  When the
software upgrade is complete, be sure to install the
cumulative PTF package.


