APAR= II09921  
CLIENT ACCESS FOR WINDOWS 95 V3R1M1 PTFS

 ** Last updated 07/11/97 **

 This informational APAR is being used to list all of the
 currently available V3R1M1 PTFs for the Client Access for
 Windows 95 client as well as PTFs needed on the AS/400.  As new
 PTFs are available or PTFs get moved onto cumulative tapes this
 Informational PTF will be updated.

 All changes that have been made to this Informational APAR
 since the last update have been marked with a vertical bar "³"
 in the left-hand column.

 Please stay current with the latest cumulative tapes to ensure
 that you have the latest support for both the AS/400 and your
 PC clients.

 The following OS/400 Licensed Programs and program temporary
 fixes (PTFs) must be installed on the AS/400 prior to
 attempting to use the Windows 95 client.  These PTFs provide
 additional function that was not available as part of the
 specified OS/400 release as well as program fixes.


 Legend:
  PTF => the ptf number for the product
  V3R1 Cum => V3R1 cum tape the ptf can be found in
  V3R2 Cum => V3R2 cum tape the ptf can be found in
  V3R6 Cum => V3R6 cum tape the ptf can be found in
  V3R7 Cum => V3R7 cum tape the ptf can be found in
     "tbd" stands for "to be determined" which means
     that the ptf is not in a cum tape yet
  CS => stands for "Character Set"
     "*" means both SBCS and DBCS environments
     "S" means SBCS environments
     "D" means DBCS environments

 PTFs required for 5763XD1 V3R1M1 Client Access for Windows 95:
 ______________________________________________________________

 It is recommended to install the following PTF on the AS/400,
 but is not a requirement.  However, it is a requirement to
 have the level of code it contains installed on the personal
 computers.

 PTF:     V3R1 Cum  V3R2 Cum  V3R6 Cum  V3R7 Cum  CS Description
 -------  --------  --------  --------  --------  -- -----------
³SF41491  tbd       tbd       tbd       tbd       *  Service Pk

 Note:  This same PTF is used on all versions of OS/400 (V3R1,
        V3R2, V3R6, and V3R7).

 PTFs required for 5763SS1 OS/400:
 _________________________________

 V3R1:
 -----

 OS/400 should be at cumulative PTF level C7044310 or later.
 Always request the latest one.

 V3R1 Client Access/400 Family - Base (5763-XA1) should be
 installed.  Note:  Client Access license management is used
 when a PC connection is established with an AS/400.

 **  Base Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 SF24885  C5249310  Graphical Access enabling
³SF41188  tbd       Graphical Access enabling
³SF39756  C7168310  PTF Support for 5763-XD1 Product
 SF35721  C7044310  Graphical Access enabling
³SF41662  tbd       Graphical Access enabling

 **  Database Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
³SF41416  tbd       Database
 SF39867  tbd       Database

 **  Server Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 SF27397  tbd       Data queues
³SF38543  C7168310  IPX/SPX
 SF35920  C7044310  Sign-on server
³SF38262  C7168310  License management
³SF41620  tbd       Data Transfer

 **  IPX/SPX (Network Extensions) Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 SF26819  tbd       for product 5733-SA1

 **  Other Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 MF13828  C7044310  PC5250 - for product 5763-999
³MF15737  tbd       Database - for product 5763-999
³MF15535  C7168310  TCP/IP - for product 5763-999

 ===============================================================

 V3R2:
 -----

 OS/400 should be at cumulative PTF level C7063320 or later.
 Always request the latest one.

 V3R2 Client Access/400 Family - Base (5763-XA1) should be
 installed.  Note:  Client Access license management is used
 when a PC connection is established with an AS/400.

 **  Base Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
³SF39757  tbd       PTF Support for 5763-XD1 Product
 SF40789  tbd       Graphical Access

 **  Database Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
³SF41466  tbd       Database
 SF39998  tbd       Database

 **  Server Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 SF36891  C7126320  Sign-on server
 SF39878  tbd       TCP/IP
³SF41227  tbd       Data Transfer


 **  Other Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 MF14230  C7126320  PC5250 - for product 5763-999
 MF15089  C7126320  TCP/IP - for product 5763-999
 MF14705  C7126320  Database - for product 5763-999
 MF15536  tbd       TCP/IP - for product 5763-999

 ===============================================================

 V3R6:
 -----
 OS/400 should be at cumulative PTF level C7140360 or later.
 Always request the latest one.

 V3R6 Client Access/400 Family - Base (5763-XA1) should be
 installed.  Note:  Client Access license management is used
 when a PC connection is established with an AS/400.

 **  Base Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 SF39759  tbd       PTF Support for 5763-XD1 Product

 **  Database Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 SF40591  tbd       Database
 SF40620  tbd       Database
³SF41902  tbd       Database

 **  Server Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 SF36892  C7051360  Sign-on server
 SF39777  tbd       TCP/IP
 SF38314  tbd       License management
 SF40262  tbd       Data Transfer

 **  Other Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 MF15630  tbd       PC5250 - for product 5716-999
³MF15736  tbd       Data Transfer - for product 5716-999
³MF15862  tbd       TCP/IP - for product 5716-999

 ===============================================================

 V3R7:
 -----

 OS/400 should be at cumulative PTF level C7056370 or later.
 Always request the latest one.

 V3R7 Client Access/400 Family - Base (5763-XA1) should be
 installed.  Note:  Client Access license management is used
 when a PC connection is established with an AS/400.

 **  Server Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
 SF36893  C7008370  Sign-on server
³SF41441  tbd       Data Transfer
³SF40705  tbd       Data Transfer & ODBC

 **  Other Host Code PTFs  **

 PTFs:    Cum       Description
 -------  --------  --------------------------------------------
³MF15982  tbd       PC5250 - for product 5716-999
 MF14618  C7056370  Data Transfer - for product 5716-999
³MF15861  tbd       TCP/IP - for product 5716-999


