5AS/400 Client Access for Windows 95/NT Client Service Pack SF40828 CD

Contents of this CD:

1. Service Pack for Client Access/400 for Windows 95/NT V3R1M2 (SF40828)
   (SERVPACK directory).
2. CA/400 Informational APARs (INFOAPAR directory)

Contents of this README:

1. Introduction
2. Service Pack Installation
3. Client Access Windows 95 32-bit Twinax Connectivity

Introduction

This Service Pack is being included in your software shipment because
it contains improved Twinax support which should allow for easier
installation and configuration of Twinax for IBM and IBM compatible Twinax
adaptors.  This Twinax support has been translated to allow
installation and configuration via English, French, German, Italian
or Spanish. All later Service Packs contain the new Twinax Support.

This Service Pack may not be the latest therefore you should check
the CA/400 home page on the internet: www.as400.ibm.com/client/cahome.htm

2. Service Pack Installation
============================

After Client Access/400 Windows 95/NT Client has been installed and
the PC has been restarted, use the following instructions to install
this Service Pack:

 a) Insert the AS/400 Client Access for Windows 95/NT Service Pack
    SF40828 CD in the compact disc drive.

 b) Click the Start button, then click Run.

 c) Type in d:\SERVPACK\SETUP  - where d is the CD-ROM drive name.

 d) Follow the instructions on the display.  Click Next to
    continue through the setup process.


3. Client Access Windows 95 32-bit Twinax Connectivity
======================================================

Client Access/400 for Windows 95/NT has improved it's Twinax support
for Windows 95 by changing from the use of DOS Terminate-Stay-Resident
programs (TSRs) to Windows 95 Virtual Device Drivers (VxDs).  Using the
new Twinax VxD support should allow for easier installation and
configuration of Twinax for IBM and IBM compatible Twinax adaptors.

This service pack CD will allow you to install and configure the new
Windows 95 twinax VxD support.

Use the following instructions to install and configure the new
Windows 95 twinax VxD support.

 a) Review Informational APAR II10307 for the latest Twinax information.
    A copy of the Informational APARs is found on this CD in the INFOAPAR
    directory.

 b) After installing the service pack in step 1, a new subdirectory
    called TWINAX will be created under the directory where Client Access
    was installed. From the TWINAX directory, print off the readme.txt
    file for your language (ENGLISH.TXT, FRENCH.TXT, GERMAN.TXT,
    ITALIAN.TXT and SPANISH.TXT).

 c) Follow the instructions in the README.TXT found in the TWINAX
    directory to complete the twinax installation process (INSTALL.EXE).




