
APAR= II09570
ETHERNET CONNECTION USING TCP/IP FAILS TO PING SUCCESSFULLY
WHEN THE AS/400 LINE DESCRIPTION FRAME SIZE WAS SET AT 1496.

** Last updated 2/25/97 **

TCP/IP ping command fails to work over Ethernet connections
when everything was configured correctly and the AS/400 Line
Description SSAP Frame size was set at 1496.

Changing the Ethernet Line Description SSAP Frame Size to
1480 (with no other changes to the configuration or setup)
allowed ping command to work.

Additional keywords: R230 R310 R320 R360
ELAN d/t2617 AA SAP Max Maximum

