
APAR= II09496  
NETSOFT NS/ROUTER V2.00I GENERAL INFORMATION AND INDEX

ERROR DESCRIPTION:

** Last updated 7/15/97 **

SNA connectivity for Client Access for Windows 95/NT client
is provided through the NetSoft NS/Router.  The following
link types are available:  802.2 (Token-Ring and ethernet),
ASYNC, SDLC, Twinax, and Netware for SAA.


CONTENTS OF THIS INFORMATIONAL APAR:
     INDEX to other NetSoft Related APARs
     VERSION information


INDEX to other NetSoft informational APARs
  Configuration Objects    . . . . . .  II09497
  Configuring, Starting, Stoping . . .  II09508
  ASYNC/SDLC Connectivity  . . . . . .  II09518
  802.2 Connectivity   . . . . . . . .  II09506
  Twinax Connectivity  . . . . . . . .  II09498
  Data Collection  . . . . . . . . . .  II09525


VERSION INFORMATION
You can determine the NetSoft Router that ships with Client
Access for Windows 95/NT by clicking on 'help' and 'about'
from the NS/Administrator panel.  Any other version of the
NS/Router is supported by the maker/integrator of the product.


Keywords:  netsoft-net-soft-w95-win95-infoapar
